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                                                                          بسمه تعالي                                 كد فرم : PR 06 F 10 ويرايش : 3
شركت مديريت توليد برق نكا
فرم استعلام بهاء الكترونيكي
	خواهشمند است آخرين‌قيمت‌پيشنهادي خود را حداكثر تا تاريخ/ /   درجدول ذيل تعيين و اعلام فرمائيد .


	رديف
	شرح كالا يا خدمات مورد استعلام
	مقدار 
	قيمت 
	قيمت‌كل
	ملاحظات

	1
	ترموکوبل وPT100 بامشخصات فنی وبه تعداد اعلام شده درجدول پیوست. 
تکمیل جدول پیوست جهت تایید فنی الزامیست.
	40عدد
	
	
	

	جمع كل به حروف:
	
	

	تذكر: زمان تحويل كالا حتماً قيد گردد، زمان اعتبار استعلام بايد بيشتر از يك ماه باشد.



اشخاص

	حقيقي

	اشخاص حقوقي


	نام و نام خانوادگي :

	نام موسسه/ شركت :


	نام فروشنده / پيمانكار:

	شماره ثبت شركت :


	كد ملي:

	كد اقتصادي :


		شناسه ملي:


	تاريخ تكميل :

	تاريخ تحويل:


	آدرس:

	كد پستي :


	تلفن :                                  نام كارشناس مربوطه و شماره همراه :                                                   نمابر :


	                                                                                   امضاي‌مدير و مهر شركت / موسسه / فروشگاه



	

	اين قسمت توسط نيروگاه تكميل خواهد شد .

در اجراي درخواست خريد شماره106344کهه در تاریخ03/ 05/1405 به اينجانب ارجاع گرديد . اين استعلام بهاء در كمال دقت تنظيم و اخذ گرديد و صحت مندرجات آن را گواهي مي‌نمايم .

تاريخ : 







   مامور خريد

	صحت مراتب فوق در مورد استعلام از شركت / مؤسسه / فروشگاه مذكور مورد تائيد ميباشد .

















رئيس اداره تداركات 

	ملاحظات:
درصورت نياز به اطلاعات فني با شماره09111548841آقاي مهندس جعفری تماس حاصل فرمائيد.
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Description

QTY

Code

Order number

Screwed — Double — Thermocouples (IRON - Const)
With connecting head made of cast Aluminium

Protecting tube made fo stainless steel 11 mm dia, 2.5 mm wall thickness.

Exchangeable sheated — measuring inset
Sheath material st.st. 6 mm dia

Thread R 1/2"

total length : lagging extension + insertion length
total length : 1885 mm

insert length : 1705 mm

lagging extension:180mm ,ungranded

10

7558711714A

106344

Screwed — Double — Thermocouples ( IRON - Const)
Without thermowell,
insertion length: 1650 mm ,probe diameterd:3mm ,ungranded

7558711820A

107131

RTD Temperature sensore , PT100 ,

Dual Element, 3-wire ,S.St sheath ,

Probe length:220mm ,

insert length : 168mm

conn:1/2 Adj

probe diameter ®:6mm,

with rotatable connector head

6Meter stainlees steel Armored cable, suitable for industrial applications

7560190012A

107140

RTD Temperature sensore,PT100,3 wire,
Without thermowell, stainless steel,
probe length:60 mm ,probe diameterd:6mm ,ungranded

7560190616A

106932

Screwed — Double — Thermocouples ( IRON — Const)
With connecting head made of cast Aluminium

Protecting tube made fo stainless steel 11 mm dia, 2.5 mm wall thickness.

Exchangeable sheated — measuring inset
Sheath material st.st. 3 mm dia

Thread R 1/2"

total length : lagging extension + insertion length
total length : 1385 mm

insert length : 1205 mm

lagging extension:180mm ,ungranded

7558711111A

106927

RTD Temperature sensore , PT100 ,Dual element,3wire, S.st probe
probe diameter ®:6mm

Brass thermowell thermowell diameter ®:9mm

Thread R 1/2"

total length : lagging extension + insertion length

total length : 320 mm

insert length :160 mm

lagging extension:160mm ,ungranded

7558712460A

106936

Screwed — Double ~ Thermocouples ( IRON — Const)
Without thermowell,
insertion length:1390 mm ,probe diameter®:6mm ,ungranded

7558713512A

106947
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